D232A, D233A, D231A top pin to GND should be VCC

VGA Connector not connected to GND

RTC C913 - + connected to -

R329 bottom pad connects to LF347 pin 9

Audio. 100Ohminstead of 10K

OPT led incoming optinal signal.- right hole (w/o CC\_ENA note) is connected to ground.

pcmcia reset is totally wrong